**SNIPER 300 CARPET MACHINE**

09 836 0937 CCREPAIRS.CO.NZ 6 TONY STREET, HENDERSON

* 0 - 300 PSI pump, 205" of water lift
* Optional 25' hose & 12" dual-jet drag wand
* 45 L solution / 45L recovery
* Heats water to 92° C
* 2000 watt in-line heater 92° C of heat for maximum cleaning productivity.
* Dual 3-stage vacuum motors offer maximum suction (205" of waterlift) to minimize drying times after extraction.
* 300 PSI adjustable pump allows the operator to dial in the correct amount of pressure for each individual job.
* Full 45L recovery and solution tanks for larger carpet cleaning jobs.

|  |  |
| --- | --- |
| **Solution Capacity** | 45L |
| **Recovery Tank Capacity** | 45L |
| **Airflow (CFM)** | 99 |
| **PSI** | 300 |
| **Vacuum Motor** | Dual 3-stage motors |
| **Electrical Draw** | 17 / 16 Amps |
| **Water Lift** | 205" |
| **Vac Hose** | 25' hose (optional) |
| **Heated** | Yes |
| **Water Heater** | 2000 Watts |
| **Power Cord** | 2, 25-foot |
| **Wheels** | 10" non-skid, non-marking rear wheels |
| **Operating Weight** | 139 lbs. |

